

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **SMILEY SQUEEGEE SPECIFICATION FOR FLEXO** | | | | |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  | |  | | --- | | PHOTO | |  |  |  |  |  |
| PRODUCT CODE | 7902-001 |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| SQUEEGEE BLADE | 16.5 INCH |  |  |  |  |  |  |
| HARDNESS | 85 ShA |  |  |  |  |  |  |
| ROTARY STEEL WIDTH | 420 MM |  |  |  |  |  |  |
| COLOUR | RED |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| PRODUCT CODE | 7902-002 |
| SQUEEGEE BLADE | 14.37 INCH |
| HARDNESS | 85 ShA |
| ROTARY STEEL WIDTH | 365 MM |
| COLOUR | RED |

